**ITRC Data Documentation**

|  |  |
| --- | --- |
| Title | ITRC Data Documentation v 1.0 |
| Document Number |  |
| Author (Organization) | Rischan Mafrur, Advanced Network Lab, CNU |
| Project Team |  |
| Creation Date | 2015-02-16 |
| Last Modified | 2015-02-17 |
| Version | 1.0 |
| Status | First Version |
| Project Link | https://github.com/rischanlab/Rfunf |
| Path of Data | C:\ITRC\_DATA (Rischan PC) |

**Revision History:**

|  |  |  |  |
| --- | --- | --- | --- |
| Modified By | Date | Version | Comments |
| Rischan | 2015-02-17 | 1.0 | First Version |
|  |  |  |  |
|  |  |  |  |

Contents

[Research Overview 4](#_Toc411980863)

[Application Data Collector 4](#_Toc411980864)

[Data Description 5](#_Toc411980865)

[On Request Data 8](#_Toc411980866)

[Simple Location Probe 8](#_Toc411980867)

[Nearby Wi-Fi Probe 9](#_Toc411980868)

[Nearby Bluetooth Probe 10](#_Toc411980869)

[Battery Probe 10](#_Toc411980870)

[Historical Data 11](#_Toc411980871)

[Call Log Probe 11](#_Toc411980872)

[Sms Log Probe 12](#_Toc411980873)

[Installed Application probe 12](#_Toc411980874)

[Hardware Info Probe 12](#_Toc411980875)

[Browser Bookmark Probe 12](#_Toc411980876)

[Browser Search Probe 13](#_Toc411980877)

[Contact Probe 13](#_Toc411980878)

[Continuous Data 13](#_Toc411980879)

[Android Sensors Data 13](#_Toc411980880)

[Running Application Probe 15](#_Toc411980881)

[Activity Probe 15](#_Toc411980882)

[Data Summarization 15](#_Toc411980883)

[Data Extraction 17](#_Toc411980884)

[Data Visualization 18](#_Toc411980885)

[Visualize the Data in Web Application 18](#_Toc411980886)

[Setup and Install Environment 22](#_Toc411980887)

[Limitation 23](#_Toc411980888)

# Research Overview

Nowadays, smartphone capability has increased significantly. Smartphone has equipped with high processor, bigger memory, bigger storage and etc. With this equipment, smartphone has capability to running complex application. Many sensor also has embedded to the smartphone. With this sensor and log capability of smartphone, we can develop many useful system or application in different domain such as healthcare (elderly monitoring system, human fall detection), transportation (monitoring road and traffic condition), personal and social behavior, environmental monitoring (pollution, weather), and etc. To develop such system, we have to collect the user personal data and then analyze it. There are two ways to collect personal data from the users based on user involvement, they are:

1. Participatory sensing
2. Opportunistic sensing

Participatory sensing means the application still need user's intervention to complete their task. The examples for such application need user to taking text input for each time period, taking picture and etc. On the other hand, opportunistic sensing means application does not need user's intervention to complete their task, users not involved in making decisions instead smart phone itself make decisions according to the sensed and stored data.

Our research focus on opportunistic sensing which is we develop application which does not need user’s intervention. To analyze the result, because of the data that we collected does not have any label so we prefer to use unsupervised learning.


In this research we develop two systems are:

1. Application data collector
2. Data extraction and visualization

Application data collector is application that we used for collecting user’s personal data. This application is android application. After we have all of data from the user, we have to extract and visualize, and also analyze it. To extract, visualize, and analyze the data, we use R programing language.

# Application Data Collector

To develop application data collector, we do not develop from scratch, we use Funf library. The Funf Open Sensing Framework is an Android-based extensible framework, originally developed at the MIT Media Lab, for doing phone-based mobile sensing. Funf provides a reusable set of functionalities enabling the collection and configuration for a broad range of data types. Funf is open sourced under the LGPL license. Figure 1 shows Funf framework can collect many of sensing from smartphone such location, movement, communication and usage, social proximity, and many more. In this document, we do not describe details about Funf architecture but we describe about the data that we have collected and how to extract, visualize and analyze it. More details about Funf architecture can be seen in the main site of Funf[[1]](#footnote-1) and also Funf developer site[[2]](#footnote-2).



# Data Description

Our application follows opportunistic sensing because we do not want to bothering user much. To do that we must define the time (interval and duration), when the application will request the data from the smartphone. Interval means how many times in second system will send data request to the smartphone. The example, we set interval 300 seconds means 5 minutes, so application will request and store the data for every 5 minutes. Duration is used in sensor data because without duration is useless to collect the sensors data. The example of duration, when we set interval 120 seconds and duration 0.07 s so the application will send data request to the smartphone for every 2 minutes and the system will record the data during 0.07 seconds.

Table 1.shows the interval and duration from each probes. Those interval and duration already tested and we thought those setting was optimum one but we can change those setting by change the value on the string.xml in android project. Figure 2a shows the string.xml file in the directory of android project and Figure 2b shows inside the string.xml file, we can change value of interval and duration in that file.

|  |  |
| --- | --- |
| C:\Users\rischan\Music\funf.png | D:\Dropbox\thesis\figures\dataviewinsmartphone.png |
| Figure 1. Funf Open Sensing Framework | Figure 3. Personal data in user’s smartphone |

To make easy for remembering, we classify the data to three of data categorization, are:

1. On Request Data (Current Data)
2. Historical Data (Saved in Android db)
3. Continuous Data (Sensor data)

On request data means we try to ask current values from android system such as location, battery, nearby Bluetooth and etc. Historical data means the data that already store in android database so we try to access and collect it, the example of historical data are contact, call log, sms log, and etc. Continuous data means we can get those data continuously such as sensor data (accelerometer, gyroscope, magnetic field, and etc). Another important thing is because we are living in time dimension space so every data has timestamp. Funf already has features to collect time, Funf using UNIX UTC (Coordinated Universal Time) which is ( Unix time or POSIX time or Unix timestamp) is the number of seconds that have elapsed since January 1, 1970. To convert UNIX time to the human readable time, we can use POSIX function in R or another programming language.

|  |  |
| --- | --- |
| D:\Dropbox\thesis\figures\ppt2\pptdata\sstringxml.JPG | D:\Dropbox\thesis\figures\ppt2\pptdata\funfsettingxml.JPG |
| (a) | (b) |
| Figure 2. (a) strings.xml file in project directory, (b) inside the string.xml file | |

Data that we collected using our application will be store in SQLite database format with (\*.db) extension, the view of data can be seen in Figure 3. To open those database, we can use SQLite browser that can be download in SQLite browser main site[[3]](#footnote-3).

## On Request Data

Table 2.shows the table of On Request Data. The table contain four columns, \_id is automatically generated by database engine, name means the name of probes (sensors), timestamp column is time when system store the data to the phone’s storage, and value is the value that returned from the sensors. On request data has four of probes are location, nearby Wi-Fi, nearby Bluetooth, and battery.

Table 2. On Request Data Table

|  |  |  |  |
| --- | --- | --- | --- |
| **\_id** | **name** | **timestamp** | **value (JSON)** |
|  | SimpleLocationProbe | Unix UTC |  |
|  | WifiProbe |  |  |
|  | BluetoothProbe |  |  |
|  | BatteryProbe |  |  |

### Simple Location Probe

Location is one of the most important information from the user. In this research, we try to get the location information from the users. The value that returned by system is like this:

{"mAccuracy":1625.0,"mAltitude":0.0,"mBearing":0.0,"mElapsedRealtimeNanos":21989372000000,"mExtras":{"networkLocationSource":"cached","networkLocationType":"cell","noGPSLocation":{"mAccuracy":1625.0,"mAltitude":0.0,"mBearing":0.0,"mElapsedRealtimeNanos":21989372000000,"mHasAccuracy":true,"mHasAltitude":false,"mHasBearing":false,"mHasSpeed":false,"mIsFromMockProvider":false,**"mLatitude":35.1837595,"mLongitude":126.9052379**,"mProvider":"network","mSpeed":0.0,"mTime":1403484137091},"travelState":"stationary"},"mHasAccuracy":true,"mHasAltitude":false,"mHasBearing":false,"mHasSpeed":false,"mIsFromMockProvider":false,"mLatitude":35.1837595,"mLongitude":126.9052379,"mProvider":"network","mSpeed":0.0,"mTime":1403484137091,"timestamp":1403484137.255}

That data which from location probes representing a geographic location. A location can consist of a latitude, longitude, timestamp, and other information such as bearing, altitude and velocity. All locations generated by the *LocationManager* are guaranteed to have a valid latitude, longitude, and timestamp (both UTC time and elapsed real-time since boot) and all other parameters are optional. In general, usually we only use latitude and longitude to define the human location, but in this data we have many of data, another data such as accuracy, bearing, altitude, and elapse real time are explained below.

**Accuracy**

Get the estimated accuracy of this location, in meters. We define accuracy as the radius of 68% confidence. In other words, if you draw a circle centered at this location's latitude and longitude, and with a radius equal to the accuracy, then there is a 68% probability that the true location is inside the circle.

**Altitude**

Get the altitude if available, in meters above the WGS 84 (World Geodetic System) reference ellipsoid. If this location does not have an altitude then 0.0 is returned. The coordinate origin of WGS 84 is meant to be located at the Earth's center of mass; the error is believed to be less than 2 cm.

**Bearing**

Get the bearing, in degrees. Bearing is the horizontal direction of travel of this device, and is not related to the device orientation. If this location does not have a bearing then 0.0 is returned.

**Elapsed Real Time**

Note that the UTC time on a device is not monotonic: it can jump forwards or backwards unpredictably. So always use *getElapsedRealtimeNanos()* when calculating time deltas. On the other hand, *getTime()* is useful for presenting a human readable time to the user, or for carefully comparing location fixes across reboot or across devices.

More details about the key and values from the location probes can be seen in Android API documentation through this link.

http://developer.android.com/reference/android/location/Location.html#

### Nearby Wi-Fi Probe

One of important information about the user is nearby Wi-Fi. This probes will collect all of Wi-Fi information which is near with user. This data also can be collected by using our application data collector. Returned value from the system is looks like:

{"BSSID":"b0:c7:45:7d:0f:7c"**,"SSID":"rischan"**,"capabilities":"[WPA2-PSK-CCMP+TKIP][ESS]","frequency":5180,**"level":-46**,"timestamp":1403476993.05}

We have 6 couple of keys and values, BSSID, SSID (Access Point name), capabilities, frequency, level, and timestamp.

**Capabilities**

Describes the authentication, key management, and encryption schemes supported by the access point.

**Frequency**

The frequency in MHz of the channel over which the client is communicating with the access point.

**Level**

The detected signal level in dBm, also known as the RSSI. Use *calculateSignalLevel(int, int)* to convert this number into an absolute signal level which can be displayed to a user.

### Nearby Bluetooth Probe

Beside of nearby Wi-Fi, one of important information related with human is nearby Bluetooth. This probes will collect all of Wi-Fi information which is near with user. The value that we get from our application looks like:

{android.bluetooth.device.extra.DEVICE":{"mAddress":"74:F0:6D:E8:ED:67"},"android.bluetooth.device.extra.NAME":"RRI-ITMS PC","android.bluetooth.device.extra.RSSI":-79,"timestamp":1404128054.397}

We have information about the device, in this case Bluetooth device address, also Bluetooth name, RSSI, and timestamp.

**android.bluetooth.device.extra.RSSI**

Used as an optional short extra field in ACTION\_FOUND intents. Contains the RSSI value of the remote device as reported by the Bluetooth hardware. Constant Value: "android.bluetooth.device.extra.RSSI“. More details about Bluetooth documentation can be seen in Android API documentation through this link

http://developer.android.com/reference/android/bluetooth/BluetoothDevice.html

### Battery Probe

Battery Probe will collect battery information from the user’s smartphone such as charging or discharging, health condition, level, and etc. The value that returned by system looks like:

{**"charge\_type":0**,**"health":2**,"icon-small":17303540, "level":89,"online":1, "scale":100,**"status":3**,"technology":"Li-ion","temperature":305,"timestamp":1403476991.281,"voltage":4138}

We have 11 couple of keys and values from those data. The description about the meaning of values of charge\_type, health, status, and voltage can be seen below:

Charge Type value meaning

* BATTERY\_PLUGED\_AC =1
* BATTERY\_PLUGGED\_USB =2
* BATTERY\_PLUGGED\_WIRELESS=4

Status value meaning

* BATTERY\_STATUS\_CHARGING =2
* BATTERY\_STATUS\_DISCHARGING =3
* BATTERY\_STATUS\_FULL =5
* BATTERY\_STATUS\_NOT\_CHARGING =4
* BATTERY\_STATUS\_UNKNOWN =1

Health values meaning

* BATTERY\_HEALTH\_COLD =7
* BATTERY\_HEALTH\_DEAD =4
* BATTERY\_HEALTH\_GOOD =2
* BATTERY\_HEALTH\_OVERHEAT =3
* BATTERY\_HEALTH\_OVER\_VOLTAGE =5
* BATTERY\_HEALTH\_UNKNOWN =1
* BATTERY\_HEALTH\_UNSPECIFIED\_FAILURE =5

**Voltage**

Integer containing the current battery voltage level. Constant Value: "voltage".

More details about Battery documentation can be seen in Android API documentation in this link http://developer.android.com/reference/android/os/BatteryManager.html

## Historical Data

Table 3. Historical Data Table

|  |  |  |  |
| --- | --- | --- | --- |
| **\_id** | **name** | **timestamp** | **value (JSON)** |
|  | CallLogProbe | Unix UTC |  |
|  | SmsProbe |  |  |
|  | ApplicationsProbe |  |  |
|  | HardwareInfoProbe |  |  |
|  | BrowserBookmarksProbe |  |  |
|  | BrowserSearchesProbe |  |  |
|  | ContactProbe |  |  |

### Call Log Probe

Asdasd

{"\_id":2172,"date":1403874310514,"duration":160,"name":"{\"ONE\_WAY\_HASH\":\"d5c7034c3a03ea8ec287f7e8f082d6ec8c07ffb1\"}","number":"{\"ONE\_WAY\_HASH\":\"d4f6776ca772a1d8fadb157ef323e906d78d8d9a,"timestamp":1403874310.514,"type":2}

Type value meaning

* INCOMING\_TYPE = 1
* OUTGOING\_TYPE = 2
* MISSED\_TYPE = 3

### Sms Log Probe

Asa

{"address":"0216441066","body":"{\"ONE\_WAY\_HASH\":\"c1f3942137da1fca36554d6c0f0dc8cd1d42e7a3\"}","body-byte-len":90,"body-token-byte-len":"3-52-16-16-","body-token-count":4,"date":1403316814524,"read":true,"thread\_id":215,"timestamp":1403316814.524,"type":1}

Type value meaning

* MESSAGE\_TYPE\_ALL =0
* MESSAGE\_TYPE\_INBOX =1
* MESSAGE\_TYPE\_SENT =2
* MESSAGE\_TYPE\_DRAFT =3
* MESSAGE\_TYPE\_OUTBOX =4
* MESSAGE\_TYPE\_FAILED =5
* MESSAGE\_TYPE\_QUEUED =6

Status value meaning

* STATUS\_NONE =-1
* STATUS\_COMPLETE =0
* STATUS\_PENDING =32
* STATUS\_FAILED =64

### Installed Application probe

Asa

{"dataDir":"**/data/data/com.lifevibes.trimapp**”,"enabled":true,"enabledSetting":0,"icon":2130837526, "installed":true,"installedTimestamp":null,"isTrusted":0,"nativeLibraryDir":"/data/data/com.lifevibes.trimapp/lib","packageName":"**com.lifevibes.trimapp**","processName":"**com.lifevibes.trimapp**”,"sourceDir":"/system/app/TrimApp\_phone\_J.apk","targetSdkVersion":17,"taskAffinity":"com.lifevibes.trimapp”,"timestamp":1403476969.264,"uid":10142}

### Hardware Info Probe

Asa

{"androidId":"5a0d4221916c50ce","bluetoothMac":"08:D4:2B:2A:05:3D","brand":"samsung","deviceId":"354257050990298","model":"SHV-E250K","timestamp":1403489373.257,"wifiMac":"08:D4:2B:2A:05:3E"}

### Browser Bookmark Probe

Asa

{"\_id":999,"bookmark":0,"created":0,"date":1403860944022,"timestamp":1403860944.022,"title":"홈 - 내학사행정","url":"http://portal.jnu.ac.kr/Education/Webservice\_S/Default.aspx","visits":125}

### Browser Search Probe

Asa

{"\_id":2,"date":1383925223295,"search":"facebook","timestamp":1383925223.295}

### Contact Probe

Asa

{"contactData":"contact\_id":3,"custom\_ringtone":"{\"ONE\_WAY\_HASH\":\"\"}","display\_name":"{\"ONE\_WAY\_HASH\":\"50bf609648d98370521094b6b724d240bd469610\"}","in\_visible\_group":1,"last\_time\_contacted":0, photo\_id":0,"send\_to\_voicemail":0,"starred":0,"times\_contacted":0,"timestamp":1404296933.626}

## Continuous Data

Table 4. Continuous Data Table

|  |  |  |  |
| --- | --- | --- | --- |
| **\_id** | **name** | **timestamp** | **value (JSON)** |
|  | LightSensorProbe | Unix UTC | {"accuracy":1,"lux":**121.0**,  "timestamp":**1402725082**.124436} |
|  | ProximitySensorProbe |  | {"accuracy":0,"distance":**8.0**,  "timestamp":**1402725082**.030173} |
|  | TemperatureSensorProbe |  |  |
|  | MagneticFieldSensorProbe |  | {"accuracy":2,"timestamp":**1402725082**.028829,"x":-**26**.939999,"y":**-8**.5199995,"z":**-24**.06} |
|  | PressureSensorProbe |  | {"accuracy":0,"pressure":**999**.82,  "timestamp":**1402725083**.016377} |
|  | ScreenProbe |  | {"screenOn":**true**,"timestamp":**1402725416**.351} |
|  | RunningApplicationsProbe |  |  |
|  | ActivityProbe |  |  |

### Android Sensors Data

The Sensor Probes that we used are light sensor, proximity sensor, temperature sensor, magnetic field sensor, and pressure sensor. Table 4. Shows the table of continuous data and on the last column, we can see the example value from each sensor probes. The data which came from android sensor have accuracy the meaning of accuracy are described below:

**Accuracy**

Meaning of accuracy values in sensors data, are:

* SENSOR\_STATUS\_ACCURACY\_HIGH means this sensor is reporting data with maximum accuracy, return value = 3.
* SENSOR\_STATUS\_ACCURACY\_LOW means this sensor is reporting data with low accuracy, calibration with the environment is needed, return value = 1
* SENSOR\_STATUS\_ACCURACY\_MEDIUM means this sensor is reporting data with an average level of accuracy, calibration with the environment may improve the readings, return value = 2.
* SENSOR\_STATUS\_UNRELIABLE means the values returned by this sensor cannot be trusted, calibration is needed or the environment doesn't allow readings, return value = 0.
* SENSOR\_STATUS\_NO\_CONTACT means the values returned by this sensor cannot be trusted because the sensor had no contact with what it was measuring (for example, the heart rate monitor is not in contact with the user), return value = -1.

The details information about android sensors can be seen in Table 5.

Table 5. Android Sensors Explanation

|  |  |  |  |
| --- | --- | --- | --- |
| Sensor | Type | Description | Common Uses |
| TYPE\_ACCELEROMETER | Hardware | Measures the acceleration force in m/s2 that is applied to a device on all three physical axes (x, y, and z), including the force of gravity. | Motion detection (shake, tilt, etc.). |
| TYPE\_LIGHT | Hardware | Measures the ambient light level (illumination) in lx.  values[0]: Ambient light level in SI lux units | Controlling screen brightness. |
| TYPE\_MAGNETIC\_FIELD | Hardware | Measures the ambient geomagnetic field for all three physical axes (x, y, z) in μT. | Creating a compass. |
| TYPE\_PRESSURE | Hardware | Measures the ambient air pressure in hPa or mbar. | Monitoring air pressure changes. |
| TYPE\_PROXIMITY | Hardware | Measures the proximity of an object in cm relative to the view screen of a device. This sensor is typically used to determine whether a handset is being held up to a person's ear.  values[0]: Proximity sensor distance measured in centimeters | Phone position during a call. |
| TYPE\_TEMPERATURE | Hardware | Measures the temperature of the device in degrees Celsius (°C). This sensor implementation varies across devices and this sensor was replaced with theTYPE\_AMBIENT\_TEMPERATURE sensor in API Level 14.  values[0]: ambient (room) temperature in degree Celsius. | Monitoring temperatures. |

### Running Application Probe

We have installed application probes which can collect the list of installed application in user’s smartphone. To know user interest we also try to collect the current applications which user used or running application.

The data from running application probes looks like:

{"duration":6.143,"taskInfo":{"baseIntent":{"mAction":"android.intent.action.MAIN","mCategories":["android.intent.category.LAUNCHER"],"mComponent":{"mClass":"kr.ac.jnu.netsys.MainActivity","mPackage":"edu.mit.media.funf.wifiscanner"}, "mPackage":"edu.mit.media.funf.wifiscanner","mWindowMode":0},"id":30,"persistentId":30},"timestamp":1402725116.144}

We have information about the name of application package which is in current running also the time usage (duration).

### Activity Probe

In our application we do not collet the accelerometer value directly but we use algorithm to determine the status of activities which are none, low, or high. We use sum of variance to detect the user activity based on accelerometer value. The details algorithm can be seen in Figure 4.

|  |
| --- |
| D:\Dropbox\thesis\figures\ppt2\activity.JPG |
| Figure 4. Activity log algorithm |

The value of activity probes that we get from the application looks like:

{"activityLevel":"none","timestamp":1402725083.715}

## Data Summarization

We have finished to collect user personal data. The all of data stored in Rischan PC using path C:\ITRC\_DATA. The data has been archived in zip format with name “itrc 2014 userdata finalpoint 20140903.zip” with size 4.25 GB. The extracted data can be accessed in path C:\ITRC\_DATA\itrc 2014 userdata finalpoint 20140903\. Extracted data contain 47 directories in different name for each student data. We have tied to looking information about those data such as the size of data from each student and starting point also ending point of data recording. The result of data summarization which contain with name of directories, size, starting point, and ending point can be seen in Table 6.

Table 6. Data Summarization from 47 students.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **No.** | **Data ID** | **Size (MB)** | **Starting Point** | **Ending Point** |
| 1. | ENFP\_0719 | 628 | 6/30/2014 8:26 | 8/20/2014 0:18 |
| 2. | ENFP\_0773 | 664 | 6/26/2014 12:34 | 8/18/2014 4:58 |
| 3. | ENFP\_2012 | 661 | 6/27/2014 6:11 | 9/2/2014 3:57 |
| 4. | ENTJ\_5868 | 6890 | 6/27/2014 5:31 | 8/13/2014 0:00 |
| 5. | ENTJ\_6454 | 121 | 6/26/2014 5:32 | 8/6/2014 18:53 |
| 6. | ENTJ\_6966 | 272 | 7/2/2014 7:24 | 8/19/2014 11:22 |
| 7. | ENTP\_5623 | 455 | 6/30/2014 4:49 | 8/19/2014 20:57 |
| 8. | ESFJ\_2301 | 145 | 6/27/2014 5:31 | 8/20/2014 2:58 |
| 9. | ESFJ\_9284 | 158 | 6/26/2014 12:34 | 8/18/2014 4:58 |
| 10. | ESFP\_0912 | 278 | 6/26/2014 5:28 | 8/18/2014 8:53 |
| 11. | ESFP\_3295 | - |  |  |
| 12. | ESFP\_4634 | 486 | 6/27/2014 5:25 | 8/20/2014 4:10 |
| 13. | ESFP\_7467 | 607 | 6/26/2014 5:27 | 8/19/2014 7:18 |
| 14. | ESTJ\_0371 | 2390 | 7/3/2014 16:21 | 8/16/2014 21:03 |
| 15. | ESTJ\_3022 | 183 | 6/26/2014 5:28 | 8/18/2014 23:22 |
| 16. | ESTJ\_5071 | 1920 | 7/2/2014 2:34 | 9/11/2014 1:49 |
| 17. | ESTJ\_5190 | 258 | 7/30/2014 6:04 | 8/24/2014 1:43 |
| 18. | ESTJ\_5824 | 173 | 6/26/2014 5:29 | 8/18/2014 3:51 |
| 19. | ESTJ\_6510 | 756 | 6/27/2014 5:30 | 8/20/2014 8:09 |
| 20. | ESTP\_4301 | 232 | 6/26/2014 5:29 | 8/20/2014 4:39 |
| 21. | ESTP\_5154 | 990 | 6/27/2014 5:31 | 8/13/2014 0:00 |
| 22. | INFP\_1993 | 432 | 6/26/2014 5:31 | 8/20/2014 0:31 |
| 23. | INTJ\_5498 | 342 | 6/26/2014 5:28 | 8/20/2014 2:49 |
| 24. | INTJ\_7906 | 312 | 6/14/2014 11:00 | 8/16/2014 23:01 |
| 25. | INTP\_3739 | 1030 | 6/27/2014 5:28 | 8/18/2014 5:58 |
| 26. | INTP\_6399 | 199 | 6/26/2014 5:29 | 8/12/2014 8:32 |
| 27. | INTP\_9712 | 180 | 6/26/2014 5:37 | 8/16/2014 18:05 |
| 28. | ISFJ\_2057 | 183 | 6/27/2014 5:32 | 8/14/2014 23:19 |
| 29. | ISFJ\_2711 | 767 | 7/31/2014 0:51 | 8/20/2014 6:59 |
| 30. | ISFJ\_7328 | 133 | 6/30/2014 7:09 | 8/19/2014 23:37 |
| 31. | ISFP\_4030 | 2380 | 6/27/2014 6:11 | 9/2/2014 3:57 |
| 32. | ISFP\_4282 | 613 | 6/27/2014 5:27 | 8/20/2014 2:46 |
| 33. | ISTJ\_0178 | 158 | 6/26/2014 5:28 | 8/19/2014 5:05 |
| 34. | ISTJ\_0386 | 284 | 6/26/2014 5:27 | 8/19/2014 7:18 |
| 35. | ISTJ\_2068 | 339 | 6/26/2014 5:29 | 8/18/2014 5:30 |
| 36. | ISTJ\_2837 | 186 | 6/27/2014 5:27 | 8/22/2014 5:41 |
| 37. | ISTJ\_3052 | 131 | 6/27/2014 5:27 | 8/20/2014 3:41 |
| 38. | ISTJ\_4659 | 325 | 7/2/2014 2:34 | 9/11/2014 1:49 |
| 39. | ISTJ\_4667 | 156 | 6/26/2014 5:29 | 8/15/2014 10:44 |
| 40. | ISTJ\_4700 | 170 | 7/3/2014 6:50 | 8/25/2014 13:08 |
| 41. | ISTJ\_4753 | 363 | 6/26/2014 5:29 | 8/18/2014 23:48 |
| 42. | ISTJ\_4968 | 95 | 7/3/2014 16:21 | 8/16/2014 21:03 |
| 43. | ISTJ\_9139 | 473 | 7/3/2014 16:21 | 8/20/2014 5:57 |
| 44. | ISTJ\_9576 | 198 | 7/4/2014 1:00 | 8/18/2014 7:12 |
| 45. | ISTP\_3948 | 500 | 6/26/2014 5:29 | 8/20/2014 1:28 |
| 46. | ISTP\_7676 | 365 | 6/27/2014 5:31 | 8/19/2014 22:11 |
| 47. | XXXX\_XXXX | 434 | 6/27/2014 5:31 | 8/21/2014 6:02 |

# Data Extraction

We have described the condition of our data that we have collected also the meaning of the value of data itself. We can use all of those data, or only one, two or more probes data according to our purpose. The value from those data is still in raw (JSON) format, to extract the most important values or values that we need we have to develop code to do that. We already develop the code for data extraction. The code can be accessed it in https://github.com/rischanlab/Rfunf in Data Extraction directory.

|  |
| --- |
| D:\Dropbox\thesis\figures\ppt2\pptdata\battery_function.JPG |
| Figure 5. Example of data extraction (Battery Probes) |

The example of data extraction using R code can be seen in Figure 5. We can see the full code in my github project that I already gave before.

# Data Visualization

## Visualize the Data in Web Application

After we collected personal user data from user’s smartphone, we need to analyze and visualize it. We also develop web application to visualize the data. We use R language to preprocessing, processing, and analysis personal user data.

Traditional tools for data analysis such as matlab, R, SPSS and etc, only support for plotting the result such as in figure with (jpeg, jpg, png) format and pdf. When we need generate document report or maybe want to expose the result in web, we have to copy the result to the web. The problem is when the data changed, we need to plot again and copy again to our document report or to the web. This application solve that problem. We use shiny library from R studio which can support to generate reproducible result for research with beautiful, interactive and responsive web layout. Figure 6. Shows the list of file in shiny project directory.




Figure 6. List of files of this framework

This application contain three main files: ui.R, server.R, and shiny.R.

1. ui.R is file that contain script to manage ui and layout of shiny application. The number of code is 202 lines with size 12 KB.
2. server.R is file that contain main script for loading, preprocessing, processing, and analysis the data, script using R language. Actually, This file contain many of functions, I just put all of functions in one file. The number of code in this file is 547 lines with size 25 KB.
3. shiny.R is config file, such as the user key, and about application configuration. This file only contain 37 lines with size 1 KB.
4. Report.Rmd this is just an example of Rmarkdown report. By using this file we can download file from plotting result (ex: regression plot) in many format such as PDF, HTML, and DOCX. The important thing is the file contain R source code and the result, so users who download that result plot they can see the source code and when they try that code in R environment will get same result. So, usually researcher call it “reproducible sample”.

The user data that we collected can be copy to folder ‘*db*’. To start this application, we need to go to parent directory before ‘*datalog’* directory. Directory ‘*datalog’* means the name of this application. This web application can be downloaded in https://github.com/rischanlab/ITRC.

To start this application using this command:

runApp("datalog",display.mode = "showcase")

Actually the purpose for creating this application is to running in server (Shiny server), but for the example, we also can run this application in desktop environment. See the video demo\_example.mov in this directory. To run this application we need some software requirements, on the next page we explain about how to setup environment in Ubuntu 12.04 or later. Example layout with this application can be seen in Figure 7. Data summary, Figure 8. Data summary using responsive table, Figure 9. Example plot of nearby Access Point, and Figure 10. Example plot of regression function that can be download as the reproducible research document.

Example Layout of this application.




Figure 7. Example plot of user data log (Installed Application in User’s smartphone)




Figure 8. Different layout to show the data (Nearby Bluetooth data)




Figure 9. Example plot of Nearby Access Point




Figure 10. An Example of regression plot that can be download for reproducible research

## Setup and Install Environment

Because of this application is for server side purpose, and to run this application, we have to setup and configure the environment. In this page, we explain about how to setup environment that can be used to run our framework.

OS requirement: **Ubuntu 12.04 or later**

Shiny Server, Currently only available for a pre-built binary for the 64-bit architecture. Running on other architectures will require building from source. Before installing Shiny Server, you’ll need to install R and the Shiny package. To install the latest version of R you should first add the CRAN repository to your system.

You can then install R using the following command:

$ sudo apt-get install r-base

NOTE: if you do not add the CRAN Debian in your Ubuntu repository this command will install the version of R corresponding to your current system version. Since this version of R may be a year or two old it is strongly recommended that you add the CRAN repositories so you can run the most up to date version of R. You’ll also need to install the Shiny R package before installing Shiny Server:

$ sudo su --c "R -e \"install.packages('shiny', repos='http://cran.rstudio.com/')\""

Once you’ve installed R and the Shiny package, execute the following commands in a terminal window to install *gdebi* (which is used to install Shiny Server and all of its dependencies) and Shiny Server.

$ sudo apt-get install gdebi-core

$ wget http://download3.rstudio.org/ubuntu-12.04/x86\_64/shiny-server-1.2.3.368-amd64.deb

$ sudo gdebi shiny-server-1.2.3.368-amd64.deb

Next Steps

Once installed, view the [Administrator’s Guide](http://rstudio.github.io/shiny-server/latest/) to learn how to manage and configure Shiny Server.

**R library needed:**

1. library(shinyapps)
2. library(shiny)
3. library(shiny)
4. library("RSQLite")
5. library("rjson")
6. library("ggplot2")
7. library("scales")
8. library("ggmap")
9. library("rmarkdown")
10. library("rmarkdown")

After the environment is ready, enter to R console and then run this command:

runApp("datalog",display.mode = "showcase")

# Limitation

Our application still need many of improvements, we have some of limitation in this application as follows:

This application does not have function that can send automatically the data from user to the server. Current version still need manually way which is using USB to copy the data from user’s phone to the PC server.

1. http://www.funf.org/ [↑](#footnote-ref-1)
2. https://code.google.com/p/funf-open-sensing-framework/wiki/FunfArchitecture [↑](#footnote-ref-2)
3. http://sqlitebrowser.org/ [↑](#footnote-ref-3)